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	AERIAL LIFTS EVALUATION


Scope and Application
To provide requirements for safe use and proper operation of aerial lifts and scissor lifts.
This applies to all locations or projects involving the use of scissor lifts, extensible boom platforms, aerial ladders, articulating boom platforms, vertical towers, or any combination thereof.
Implementation
[bookmark: _Int_JQuWpwp1]It is the responsibility of the management to administer this procedure.  All employees and contractors involved are responsible for adhering to this policy.
General Requirements
1.0 Equipment Requirements
A. Aerial lifts acquired for use after January 22, 1973, shall be designed and constructed in conformance with the applicable requirements of the American National Standards for “Vehicle Mounted Elevating and Rotating Work Platforms,” ANSI A92.2-1969, including appendix. Procedures.
B. Lifts must utilize standard guardrails unless specifically required by the manufacturer.

2.0 Equipment Modifications
A. [bookmark: _Int_TTw33oF7]Never field modify an aerial lift for use other than those intended by the manufacturer.
B. Any modifications for use other than those intended by the manufacturer must have authorization from the manufacturer, which is certified in writing. 
C. Alteration of the insulated portion of an aerial lift that may reduce the insulating value is not permitted.

3.0 Documentation
A. The manufacturer’s operating instruction manual must be available on site.
B. File the following documents in the Shop/Project Health and Safety File.
1. Copy of the cover page of the Manufacturer's Operation Manual.
2. Training documentation.
3. List of authorized employees.
4. Daily inspections.



4.0 Operator Training
A. [bookmark: _Int_LluIBLQz]Only trained and authorized personnel are allowed to operate aerial lifts.

5.0 Maintenance and Inspection
A. Inspect the unit for unsafe conditions each day prior to use. Units damaged or weakened from any cause must be taken out of service until repairs are done.
B. Test the lift controls every day, prior to operation, to ensure they are in safe working order.

6.0 Fall Protection
A. Wear fall protection in the form of a full body harness and lanyard attached to the manufacturer’s prescribed anchorage point. 
B. Fall protection is not required for scissors.

7.0 Set Up
A. Requires that both lower and platform controls be plainly marked as to their function.
B. Survey the route to be traveled immediately prior to the work trip to check for overhead obstructions, holes in pavement, slopes, ditches, or other potential hazards.
C. Set the braking system before elevating the basket.
D. Install wheel chocks before using an aerial lift on an incline, provided they can be safely installed.
E. Electrically ground or barricade aerial lifts when working near energized lines or equipment and consider the lift to be energized equipment.

8.0 Operation
A. Stand firmly on the floor of the basket when working from an aerial lift. Sitting or climbing on the edge of the basket and/or use of planks, ladders, or other devices for work position are prohibited.
B. Never exceed the boom and basket load limits set by the manufacturer.
C. [bookmark: _Int_Jb0Enzzy]Do not pass equipment between a pole or structure and an aerial lift while an employee working from the basket is within reaching distance of energized conductors or equipment that are not covered with insulating protective equipment. 
D. Do not operate lower controls unless permission has been obtained from the employee in the basket, except in case of emergency. 
E. Aerial lift trucks must not be moved when the boom is not secured in a traveling position and with workers in the basket.
F. Aerial ladders must be secured in the traveling position by the locking device on top of the truck cab, and the manually operated device at the base of the ladder before the truck is moved for travel.
G. Belting off to another structure or pole, while working from the lift is not permitted.




9.0 Documentation Summary
A. The Risk Management Center is to be used to document all information including the following:

	Documents
	Risk Management Center Location

	Written Aerial Lift Safety Program 
	My ContentTM

	Training Documentation including: 
- Classroom training and training course completed
- Sign-in sheets
- Quizzes
- Skills evaluations
- Operator Certificates
	Training TrackTM application

	Pre-shift Inspection Checklists
	My ContentTM

	Safety Observations
	Job Hazard Analysis/ Safety Observation ToolTM

	Near misses
	Incident TrackTM

	Accidents and claims
	Incident TrackTM

	Supplier and manufacturer Certificates of Insurance
	COI TrackTM

	Safety Data Sheets
	SDS TrackTM
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