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	FORMWORK


Despite the simplicity or difficulty of formwork requirements, safety must be included in every phase and activity of its construction.  Pre-job planning should incorporate various types of forming systems and engineering requirements, as well as material storage, handling, erection, and stripping techniques.
Formwork requires repeated handling and re-use of materials and equipment.  A well-organized storage area saves accidents and reduces material waste.  Stockpile materials in an orderly manner to:
1. Prevent piles from toppling.
2. Keep storage areas clean to eliminate tripping and fire hazards.
3. Avoid painful puncture wounds by pulling used nails from lumber.
Always be alert for overhead electrical lines when using power equipment to handle materials.
Since most forming materials are handled by hand, remember to lift loads with your legs, not your back.  If the load is too heavy, get "help", not "hurt".  Before carrying a load, make sure the path is clear and watch where you step.  Wearing the proper gloves can protect your hands from splinters and other minor injuries.
As forms get higher, standard guard rails become a part of their construction.  Guard rails are required on all open sides and ends of platforms more than 10 feet in height, and on any scaffold platform less than 45 inches wide and over 4 feet high.
To ensure that no materials have been removed or omitted, always check the entire form system prior to concrete placement.  Keep in mind that mechanical vibration can increase concrete pressure by approximately 35% and loosen or disengage forming hardware.
Operators of equipment and workers on the ground should have protection against weather, falling objects, swinging loads, and similar hazards.
 Serious form failures continue to recur due to the same old reasons:
1. Safe shoring procedures were not followed.
2. Formwork design was faulty.
3. Concentrated overloading exceeded design strength.
4. Poor workmanship.
5. Shortcuts.
6. Lack of competent supervision.
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	SAFETY TALK SIGN IN SHEET



This form documents that the training specified above was presented to the listed participants. By signing below, each participant acknowledges receiving this training.

Organization:												          
		
Trainer:					 Trainer’s Signature:					

Class Participants:

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			

Name:					 Signature:				 Date:			
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